--lpm_compare DEVICE_FAMILY="Cyclone IV E" LPM_WIDTH=3 ONE_INPUT_IS_CONSTANT="YES" aeb dataa datab
--VERSION_BEGIN 10.1SP1 cbx_cycloneii 2011:01:19:21:13:40:SJ cbx_lpm_add_sub 2011:01:19:21:13:40:SJ cbx_lpm_compare 2011:01:19:21:13:40:SJ cbx_mgl 2011:01:19:21:15:40:SJ cbx_stratix 2011:01:19:21:13:40:SJ cbx_stratixii 2011:01:19:21:13:40:SJ  VERSION_END


-- Copyright (C) 1991-2011 Altera Corporation
--  Your use of Altera Corporation's design tools, logic functions 
--  and other software and tools, and its AMPP partner logic 
--  functions, and any output files from any of the foregoing 
--  (including device programming or simulation files), and any 
--  associated documentation or information are expressly subject 
--  to the terms and conditions of the Altera Program License 
--  Subscription Agreement, Altera MegaCore Function License 
--  Agreement, or other applicable license agreement, including, 
--  without limitation, that your use is for the sole purpose of 
--  programming logic devices manufactured by Altera and sold by 
--  Altera or its authorized distributors.  Please refer to the 
--  applicable agreement for further details.



--synthesis_resources = 
SUBDESIGN cmpr_gs8
( 
	aeb	:	output;
	dataa[2..0]	:	input;
	datab[2..0]	:	input;
) 
VARIABLE 
	aeb_result_wire[0..0]	: WIRE;
	aneb_result_wire[0..0]	: WIRE;
	data_wire[7..0]	: WIRE;
	eq_wire	: WIRE;

BEGIN 
	aeb = eq_wire;
	aeb_result_wire[] = (! aneb_result_wire[]);
	aneb_result_wire[] = (data_wire[0..0] # data_wire[1..1]);
	data_wire[] = ( datab[2..2], dataa[2..2], datab[1..1], dataa[1..1], datab[0..0], dataa[0..0], (data_wire[6..6] $ data_wire[7..7]), ((data_wire[2..2] $ data_wire[3..3]) # (data_wire[4..4] $ data_wire[5..5])));
	eq_wire = aeb_result_wire[];
END;
--VALID FILE
