#============================================================
# Build by Terasic System Builder
#============================================================

set_global_assignment -name FAMILY "Cyclone IV E"
set_global_assignment -name DEVICE EP4CE115F29C8
set_global_assignment -name TOP_LEVEL_ENTITY "DE2_115_ADDA"
set_global_assignment -name ORIGINAL_QUARTUS_VERSION 9.1
set_global_assignment -name LAST_QUARTUS_VERSION "10.1 SP1"
set_global_assignment -name PROJECT_CREATION_TIME_DATE "09:58:27 JULY 12,2010"
set_global_assignment -name DEVICE_FILTER_PIN_COUNT 780
set_global_assignment -name DEVICE_FILTER_SPEED_GRADE 8
set_global_assignment -name SDC_FILE DE2_115_ADDA.SDC

#============================================================
# CLOCK
#============================================================
set_location_assignment PIN_Y2 -to CLOCK_50
set_instance_assignment -name IO_STANDARD "3.3-V LVTTL" -to CLOCK_50
set_location_assignment PIN_AG14 -to CLOCK2_50
set_instance_assignment -name IO_STANDARD "3.3-V LVTTL" -to CLOCK2_50
set_location_assignment PIN_AG15 -to CLOCK3_50
set_instance_assignment -name IO_STANDARD "3.3-V LVTTL" -to CLOCK3_50

#============================================================
# I2C for HSMC 
#============================================================
set_location_assignment PIN_B7 -to I2C_SCLK
set_instance_assignment -name IO_STANDARD "3.3-V LVTTL" -to I2C_SCLK
set_location_assignment PIN_A8 -to I2C_SDAT
set_instance_assignment -name IO_STANDARD "3.3-V LVTTL" -to I2C_SDAT

#============================================================
# HSMC, HSMC connect to ADA - High Speed ADC/DAC
#============================================================
set_location_assignment PIN_D27 -to DAC_DA[0]
set_instance_assignment -name IO_STANDARD "2.5 V" -to DAC_DA[0]
set_location_assignment PIN_F24 -to DAC_DB[0]
set_instance_assignment -name IO_STANDARD "2.5 V" -to DAC_DB[0]
set_location_assignment PIN_D28 -to DAC_DA[1]
set_instance_assignment -name IO_STANDARD "2.5 V" -to DAC_DA[1]
set_location_assignment PIN_F25 -to DAC_DB[1]
set_instance_assignment -name IO_STANDARD "2.5 V" -to DAC_DB[1]
set_location_assignment PIN_E27 -to DAC_DA[2]
set_instance_assignment -name IO_STANDARD "2.5 V" -to DAC_DA[2]
set_location_assignment PIN_D26 -to DAC_DB[2]
set_instance_assignment -name IO_STANDARD "2.5 V" -to DAC_DB[2]
set_location_assignment PIN_E28 -to DAC_DA[3]
set_instance_assignment -name IO_STANDARD "2.5 V" -to DAC_DA[3]
set_location_assignment PIN_C27 -to DAC_DB[3]
set_instance_assignment -name IO_STANDARD "2.5 V" -to DAC_DB[3]
set_location_assignment PIN_F27 -to DAC_DA[4]
set_instance_assignment -name IO_STANDARD "2.5 V" -to DAC_DA[4]
set_location_assignment PIN_F26 -to DAC_DB[4]
set_instance_assignment -name IO_STANDARD "2.5 V" -to DAC_DB[4]
set_location_assignment PIN_F28 -to DAC_DA[5]
set_instance_assignment -name IO_STANDARD "2.5 V" -to DAC_DA[5]
set_location_assignment PIN_E26 -to DAC_DB[5]
set_instance_assignment -name IO_STANDARD "2.5 V" -to DAC_DB[5]
set_location_assignment PIN_G27 -to DAC_DA[6]
set_instance_assignment -name IO_STANDARD "2.5 V" -to DAC_DA[6]
set_location_assignment PIN_G25 -to DAC_DB[6]
set_instance_assignment -name IO_STANDARD "2.5 V" -to DAC_DB[6]
set_location_assignment PIN_G28 -to DAC_DA[7]
set_instance_assignment -name IO_STANDARD "2.5 V" -to DAC_DA[7]
set_location_assignment PIN_G26 -to DAC_DB[7]
set_instance_assignment -name IO_STANDARD "2.5 V" -to DAC_DB[7]
set_location_assignment PIN_K27 -to DAC_DA[8]
set_instance_assignment -name IO_STANDARD "2.5 V" -to DAC_DA[8]
set_location_assignment PIN_H25 -to DAC_DB[8]
set_instance_assignment -name IO_STANDARD "2.5 V" -to DAC_DB[8]
set_location_assignment PIN_K28 -to DAC_DA[9]
set_instance_assignment -name IO_STANDARD "2.5 V" -to DAC_DA[9]
set_location_assignment PIN_H26 -to DAC_DB[9]
set_instance_assignment -name IO_STANDARD "2.5 V" -to DAC_DB[9]
set_location_assignment PIN_M27 -to DAC_DA[10]
set_instance_assignment -name IO_STANDARD "2.5 V" -to DAC_DA[10]
set_location_assignment PIN_K25 -to DAC_DB[10]
set_instance_assignment -name IO_STANDARD "2.5 V" -to DAC_DB[10]
set_location_assignment PIN_M28 -to DAC_DA[11]
set_instance_assignment -name IO_STANDARD "2.5 V" -to DAC_DA[11]
set_location_assignment PIN_K26 -to DAC_DB[11]
set_instance_assignment -name IO_STANDARD "2.5 V" -to DAC_DB[11]
set_location_assignment PIN_K21 -to DAC_DA[12]
set_instance_assignment -name IO_STANDARD "2.5 V" -to DAC_DA[12]
set_location_assignment PIN_L23 -to DAC_DB[12]
set_instance_assignment -name IO_STANDARD "2.5 V" -to DAC_DB[12]
set_location_assignment PIN_K22 -to DAC_DA[13]
set_instance_assignment -name IO_STANDARD "2.5 V" -to DAC_DA[13]
set_location_assignment PIN_L24 -to DAC_DB[13]
set_instance_assignment -name IO_STANDARD "2.5 V" -to DAC_DB[13]
set_location_assignment PIN_H23 -to DAC_WRT_A
set_instance_assignment -name IO_STANDARD "2.5 V" -to DAC_WRT_A
set_location_assignment PIN_M25 -to DAC_WRT_B
set_instance_assignment -name IO_STANDARD "2.5 V" -to DAC_WRT_B
set_location_assignment PIN_H24 -to DAC_MODE
set_instance_assignment -name IO_STANDARD "2.5 V" -to DAC_MODE
set_location_assignment PIN_G23 -to DAC_CLK_A
set_instance_assignment -name IO_STANDARD "2.5 V" -to DAC_CLK_A
set_location_assignment PIN_J27 -to OSC_SMA_ADC4
set_instance_assignment -name IO_STANDARD "2.5 V" -to OSC_SMA_ADC4
set_location_assignment PIN_G24 -to DAC_CLK_B
set_instance_assignment -name IO_STANDARD "2.5 V" -to DAC_CLK_B
set_location_assignment PIN_J28 -to SMA_DAC4
set_instance_assignment -name IO_STANDARD "2.5 V" -to SMA_DAC4
set_location_assignment PIN_T25 -to ADC_OEB_A
set_instance_assignment -name IO_STANDARD "2.5 V" -to ADC_OEB_A
set_location_assignment PIN_T26 -to ADC_OEB_B
set_instance_assignment -name IO_STANDARD "2.5 V" -to ADC_OEB_B
set_location_assignment PIN_J25 -to ADC_DB[13]
set_instance_assignment -name IO_STANDARD "2.5 V" -to ADC_DB[13]
set_location_assignment PIN_U25 -to ADC_DA[13]
set_instance_assignment -name IO_STANDARD "2.5 V" -to ADC_DA[13]
set_location_assignment PIN_J26 -to ADC_DB[12]
set_instance_assignment -name IO_STANDARD "2.5 V" -to ADC_DB[12]
set_location_assignment PIN_U26 -to ADC_DA[12]
set_instance_assignment -name IO_STANDARD "2.5 V" -to ADC_DA[12]
set_location_assignment PIN_L27 -to ADC_DB[11]
set_instance_assignment -name IO_STANDARD "2.5 V" -to ADC_DB[11]
set_location_assignment PIN_L21 -to ADC_DA[11]
set_instance_assignment -name IO_STANDARD "2.5 V" -to ADC_DA[11]
set_location_assignment PIN_L28 -to ADC_DB[10]
set_instance_assignment -name IO_STANDARD "2.5 V" -to ADC_DB[10]
set_location_assignment PIN_L22 -to ADC_DA[10]
set_instance_assignment -name IO_STANDARD "2.5 V" -to ADC_DA[10]
set_location_assignment PIN_V25 -to ADC_DB[9]
set_instance_assignment -name IO_STANDARD "2.5 V" -to ADC_DB[9]
set_location_assignment PIN_N25 -to ADC_DA[9]
set_instance_assignment -name IO_STANDARD "2.5 V" -to ADC_DA[9]
set_location_assignment PIN_V26 -to ADC_DB[8]
set_instance_assignment -name IO_STANDARD "2.5 V" -to ADC_DB[8]
set_location_assignment PIN_N26 -to ADC_DA[8]
set_instance_assignment -name IO_STANDARD "2.5 V" -to ADC_DA[8]
set_location_assignment PIN_R27 -to ADC_DB[7]
set_instance_assignment -name IO_STANDARD "2.5 V" -to ADC_DB[7]
set_location_assignment PIN_P25 -to ADC_DA[7]
set_instance_assignment -name IO_STANDARD "2.5 V" -to ADC_DA[7]
set_location_assignment PIN_R28 -to ADC_DB[6]
set_instance_assignment -name IO_STANDARD "2.5 V" -to ADC_DB[6]
set_location_assignment PIN_P26 -to ADC_DA[6]
set_instance_assignment -name IO_STANDARD "2.5 V" -to ADC_DA[6]
set_location_assignment PIN_U27 -to ADC_DB[5]
set_instance_assignment -name IO_STANDARD "2.5 V" -to ADC_DB[5]
set_location_assignment PIN_P21 -to ADC_DA[5]
set_instance_assignment -name IO_STANDARD "2.5 V" -to ADC_DA[5]
set_location_assignment PIN_U28 -to ADC_DB[4]
set_instance_assignment -name IO_STANDARD "2.5 V" -to ADC_DB[4]
set_location_assignment PIN_R21 -to ADC_DA[4]
set_instance_assignment -name IO_STANDARD "2.5 V" -to ADC_DA[4]
set_location_assignment PIN_V27 -to ADC_DB[3]
set_instance_assignment -name IO_STANDARD "2.5 V" -to ADC_DB[3]
set_location_assignment PIN_R22 -to ADC_DA[3]
set_instance_assignment -name IO_STANDARD "2.5 V" -to ADC_DA[3]
set_location_assignment PIN_V28 -to ADC_DB[2]
set_instance_assignment -name IO_STANDARD "2.5 V" -to ADC_DB[2]
set_location_assignment PIN_R23 -to ADC_DA[2]
set_instance_assignment -name IO_STANDARD "2.5 V" -to ADC_DA[2]
set_location_assignment PIN_U22 -to ADC_DB[1]
set_instance_assignment -name IO_STANDARD "2.5 V" -to ADC_DB[1]
set_location_assignment PIN_T21 -to ADC_DA[1]
set_instance_assignment -name IO_STANDARD "2.5 V" -to ADC_DA[1]
set_location_assignment PIN_V22 -to ADC_DB[0]
set_instance_assignment -name IO_STANDARD "2.5 V" -to ADC_DB[0]
set_location_assignment PIN_T22 -to ADC_DA[0]
set_instance_assignment -name IO_STANDARD "2.5 V" -to ADC_DA[0]
set_location_assignment PIN_V23 -to ADC_CLK_B
set_instance_assignment -name IO_STANDARD "2.5 V" -to ADC_CLK_B
set_location_assignment PIN_Y27 -to ADC_OTR_B
set_instance_assignment -name IO_STANDARD "2.5 V" -to ADC_OTR_B
set_location_assignment PIN_V24 -to ADC_CLK_A
set_instance_assignment -name IO_STANDARD "2.5 V" -to ADC_CLK_A
set_location_assignment PIN_Y28 -to ADC_OTR_A
set_instance_assignment -name IO_STANDARD "2.5 V" -to ADC_OTR_A

#============================================================
# End of pin assignments by Terasic System Builder
#============================================================


set_global_assignment -name MISC_FILE "E:/My_design/345/DE2_115_ADDA.dpf"
set_global_assignment -name QIP_FILE nco91.qip
set_global_assignment -name QIP_FILE pll.qip
set_global_assignment -name QIP_FILE lpm_add.qip
set_global_assignment -name PARTITION_NETLIST_TYPE SOURCE -section_id Top
set_global_assignment -name PARTITION_COLOR 16764057 -section_id Top
set_global_assignment -name LL_ROOT_REGION ON -section_id "Root Region"
set_global_assignment -name LL_MEMBER_STATE LOCKED -section_id "Root Region"
set_global_assignment -name SIGNALTAP_FILE stp1.stp
set_global_assignment -name ENABLE_SIGNALTAP OFF
set_global_assignment -name USE_SIGNALTAP_FILE stp1.stp
set_global_assignment -name TIMEQUEST_MULTICORNER_ANALYSIS ON
set_global_assignment -name TIMEQUEST_DO_CCPP_REMOVAL ON
set_global_assignment -name MIN_CORE_JUNCTION_TEMP 0
set_global_assignment -name MAX_CORE_JUNCTION_TEMP 85
set_global_assignment -name NOMINAL_CORE_SUPPLY_VOLTAGE 1.2V
set_global_assignment -name USE_CONFIGURATION_DEVICE OFF
set_global_assignment -name VERILOG_FILE DE2_115_ADDA_TOP.v
set_global_assignment -name MISC_FILE "E:/My_design/DE2_115_ADDA/DE2_115_ADDA.dpf"
set_global_assignment -name PARTITION_FITTER_PRESERVATION_LEVEL PLACEMENT_AND_ROUTING -section_id Top
set_global_assignment -name QIP_FILE mynco.qip
set_global_assignment -name QIP_FILE filter.qip
set_instance_assignment -name PARTITION_HIERARCHY root_partition -to | -section_id Top